**Package**:eB DataLayer for iRINGTools

**Package Version**:1.00.00

**Package Date**: 6/21/12

**QA/CM Contact**:

**Application Contact:** Hahn Le

**Overview:**

The eB DataLayer is an iRINGTools DataLayer, and follows the standard deployment for iRINGTools DataLayers. The process will still be detailed below to help deploy the DataLayer onto an iRINGTools Adapter Services server.

**Prerequisites:**

1. iRINGTools Adapter 2.04.xx
2. eB Director from

\\chist95004\edrive\Hirantha\Software\BentleyDownloads\ebi150302261en\Client Installation\Director

**Installation Steps:**

1. *Preparation. Copy the following files to the server:*

* ebDataLayer-1.0.0.zip
* install-eb-datalayer.ps1
* install-eb-datalayer -with-log.ps1

1. *Execution*
2. *First time:*

* Open PowerShell console as Administrator
* Run script “install-eb-datalayer -with-log.ps1” in the console
* Inspect log “%temp%\install-eb-datlayer.log” for any error

1. *After context and application have been created in Adapter Manager:*

* Open PowerShell console as Administrator
* Run script “install-eb-datalayer -with-log.ps1” in the console with context, application, and community name as parameters. For example:

.\ install-eb-datalayer -with-log.ps1 MPower Pilot BechtelPreProd

* Inspect log “%temp%\install-eb-datlayer.log” for any error
* Make any changes to configuration files as necessary